## Pfane EcoCell

The new way to produce pure metals directly from granules. No melting, no harsh acids, solar powered and hydrogen producing.

### We want every electronics recycler in the world to be circular and CO2 negative.

Pre-ORDER NOW

## 7% of the Worlds CO2
is Produced By The Metal Melting Industry.

Not including Transport

### The Current Method

1. Metal in the form of Granules, shreds, scrap or oxides are collected from numerous different producers (Co2 added due to transport)
2. Metals are sent to processors to be melted and refined, metals are oxides are mixed with fluxes and carbon to create impure metal slabs that can act as anodes. (burns fuel, releases tons of carbon plus the carbon from transporting the scrap granules)
3. Huge tanks of harsh sulfuric acid or other catalysts are used along with DC current (100 - 200amps per meter) to elecrolyze impure metal sheets into pure metal cathodes. (most energy comes from a lacking grid and uses fossil fuels to produce the power = more CO2)
4. Pure metal sheets are sent to various manufacturers to be melted or used in manufacturing of various metal products. (added CO2 From shipping, re melting, power used to create new products)
Approximately 10 tons of CO2
is generated to create products from just ONE TON of NEW OR RECYCLED Metal.

### The Pfane Way

1. Manufacturers and producers send their scraps to Pfane or Pfane Partner facilities using the Eco Cell technology.
2. Metal is ground in machines that use clean renewable sources for energy
3, The ground metal is placed in our patent pending, solar powered electrolysis metal refining cells which can be formatted to produce either sheets or 3mm pure metal wire (coming soon)
4. The process uses regular table vinegar as the catalyst, which is compensated by a massive surface area made available from the granules, turning water back into Hydrogen and Oxygen, where Hydrogen can be collected and used to supliment power for the recycling line. (no sacraficial metal or sulpher is used in the anode)
5. Products such as copper wire, can be perfected inhouse, spooled and sold to industry.
6. Remaining metal granules are now easily sorted through gravity seperation or extremely small scale precious metal refining methods.
With the production of products onsite, plus savings from shipping and lack of melting.
More than 13 Tons Of CO2 Is Saved
from entering the atmosphere for EACH ONE TON of metal being recycled.

DOWNLOAD THE PFANE CO2 PDF

## Carbon Negative Refining

- System
- FeedStock
- Results
- Left Over Granules
- Further Refining

- uses 0.3 to 0.5 amps per kg of metal at 1.2 volts
- catalyst made inhouse inexpensively from standard table vinegar
- pure 9999 copper cathode or wire is produced
- no toxic gasses emmitted
- no greenhouse gasses emmitted
- generates hydrogen and oxygen
- low voltage DC current is non lethal and safe to handle with care.

PREORDER NOW

- Can accept 1cm down to 0.001mm granules and metal dust
- 80% clean metal works fine.
- plastics or fiber contamination does not matter
- mixed precious metals material
- requires 60% of the content to be copper.
- note: larger material may require higher amperage system is rated at 2mm granule size.

PREORDER NOW

- in 20 minutes can see 9999s copper building up on cathode.
- depending on sunlight or power source and copper content cells will complete transfer inside 24 days.
- cathode copper can be sold to industry as is or made into foil products
- wire generating cathode can produce 3mm x 3mm x 10 r 20 meters of solid copper wire in around 3 hours. (special order cathode)

PREORDER NOW

- Granules left over contain no less than 5% copper
- as seen in the photo, predominant gold foils, silver, steel and plastic remain
- much easier to sort
- maximum value acheived
- exremely small amount of inhouse refining required (whatever method you preffer)

PREORDER NOW

- 2kg lab cell can be used to refine precious metals into jewelery grade metals
- seperate solution to use for electrolytic conversion of precious metals (sold seperately)
- 100% inhouse, small or large scale production,
- Greatly Increases revenue
- reduces risk of sale of unclean granules.
- Safe and Environmentally conscious.

PREORDER NOW

## Delivery To Begin - Q1 2023

#### ECO Cell 250 - PILOT

> Save humanity from up to
> 250 tons
> of CO2 per month.

5x ~50kg per month modules
40 new solar panels 500w each 12v DC (132sqM)
Eco Cell mounting rack
Solar roof mounting kit
Standard Stainless Steel Cathodes
Produces Approx 250kg pure Cu / day
Solar requires 132 square meters roof
Eco Cells require 5 m x 90cm for rack and cells
(delivery / setup not included)

PREORDER

#### $29000 USD

#### Eco Cell 500

> Save humanity from up to
> 500 tons
> of CO2 per month.

10x ~50kg per month modules
100 new solar panels 500w each 12v DC (220sqM)
Eco Cell mounting rack
solar roof mounting kit
Standard Stainless Steel Cathodes
Produces Approx 500kg pure Cu / day
Solar requires 220 square meters roof
Eco Cells require 10m x 90cm for rack and cells or 5m x 2m
(delivery / setup not included)

PREORDER

#### $49500 USD

#### eco cell 1000

> Saves humanity from up to
> 1 MEGA TON
> of CO2 per month.

20x ~50kg per month modules
200 new solar panels 500w each 12v DC (440sqM)
Eco Cell mounting rack
solar roof mounting kit
Standard Stainless Steel Cathodes
Produces Approx 1Ton pure Cu / day
Solar requires 440 square meters roof
Eco Cells require 10m x 2m for rack and cells or 5m x 4.5m
(delivery / setup not included)

PREORDER

#### $94500 USD

## 20 System Pilot Program

We are offering 20 fabricated run full systems of the EcoCell250 model WorldWide.
This is your chance to jump to the front of the line.

### 5 Modules

One refining cell and setup for copper primary granule refinement. Including metal support for 5 modules. Connections and Setup Guide. To make ~250 kg of 99's copper in 24 days of sunlight.

### The Recipe

Simple recipe for making the vinegar copper catalyst

### Solar System

4x 500watt panels for each module (20 panels total) plus roof mounts for standard pitch shop roof.

### Standby

5 x 30v-10amp standby DC Power supply provides just the right power overnight to keep your copper from collecting back into solution.

### 2 Year Warantee

Full part replacement warantee for 2 years from original delivery date. Covering all Cell Components excluding electrical components.

### Honorable Mention

You, and 19 other companies will earn a spot on the Pfane Environmental Association Partners list and take part in the promotion though our sponsored Google Ads Campaign.

## BE PART OF THE 20 SYSTEM PILOT

Get 10% off full system price, Pay Just $10,000 USD deposit. (offer only available to the next 16 signups)

I WANT TO OWN A PILOT SYSTEM